                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


http://www.thingiverse.com/thing:1671517
Mostly Printed CNC "MPCNC" BURLY J-25.4mm = 1" OD by Allted is licensed under the Creative Commons - Attribution - Non-Commercial - Share Alike license.
http://creativecommons.org/licenses/by-nc-sa/3.0/

# Summary

#Mostly Printed CNC / Multi-Tool
These parts are for *25.4mm* OD conduit.
25mm OD here- http://www.thingiverse.com/thing:790533
23.5mm OD here- https://www.thingiverse.com/thing:724999

**Changelog**
10/15/18 - BURLY Center Revisions
3/19/18 - New foot design.
5/9/17 - New XYZ Part to allow for T8 Leadscrew driven Z axis.
7/13/16 - New Roller Assemblies. New size added.
5/25/16 - New Center and Z Axis assemblies, universal tool mount.
4/24/16 - New Corner assembly.

**The "MPCNC" a minimal cost CNC machine that is easily sourced worldwide and can easily swap out its functionality. **

For More Information and to purchase parts please visit,
https://www.V1Engineering.com/   

Printing info  
https://www.V1engineering.com/blog/parts/  

**Please ask all questions in the forums, or help out if you can.**
The forums are extremely active and very beginner friendly.
https://www.v1engineering.com/forum/

The only special tools needed are a hacksaw, and a drill to for 4 holes.   
   
This can be easily expanded to almost any length, width, and depth depending on rigidity required. Shorter lengths = more rigid.  This is built using hardware store emt conduit (In the US it is sold as 3/4" (ID)), or as an upgrade you can use stainless steel tubing.

 Most woods and plastics should be no problem, https://youtu.be/Ub2qablc-GE. I milled Aluminum with a footprint of 23.5in x 32in x 4in.  Aluminum works well https://youtu.be/BRFeZESDo4k Yes, even some Steel https://youtu.be/1CX3qui0-Yo.

You can switch the spindle out with a drag knife, laser, Extruder, ect, making it a great prototyping multi-tool. By adding length and depth It could easily be used to shape large easily milled things like wood, foam, or plastics. Keep it small for metals.   

#Add Ons  

Dual End Stop Mounts
https://www.thingiverse.com/thing:2847042  

MK8 MK9 extruder mount 3D printer  
http://www.thingiverse.com/thing:868983  

Dewalt DW660 Mount  
http://www.thingiverse.com/thing:944952  
http://amzn.to/1D7xByM  

DW660 perpendicularity tester
http://www.thingiverse.com/thing:1525661
  
Pen Mount
http://www.thingiverse.com/thing:1612207  

Blank Tool Mounts  
http://www.thingiverse.com/thing:805803

Laser (Leo69) Mount
http://www.thingiverse.com/thing:1636811

If what you are looking for isn't here search "MPCNC"